Last saved by: Michael Marshall

+++ EDITOR NOTE: Items in red to be addressed on a per project basis +++

SECTION 08 3200

SLIDING GLASS DOORS
PART 1  GENERAL
1.01	SECTION INCLUDES
A.	Sliding doors and frames.
1.02	RELATED REQUIREMENTS
A.	Section 07 9005 - Joint Sealers:  Perimeter sealant and backup materials.
B.	Section 08 1100 - Aluminum Doors and Frames.
C.	Section 08 3201 - Lift-Sliding and Sliding-Folding Glass Doors.
D.	Section 08 4413 - Glazed Aluminum Curtain Walls.
E.	Section 08 5113 - Aluminum Windows.
F.	Section 08 6300 - Metal-framed Skylights.
G.	Section 08 8000 - Glazing
H.	Section 09 9000 - Painting and Coating.
1.03	REFERENCE STANDARDS
1.04	ADMINISTRATIVE REQUIREMENTS
A.	System Supplier to provide Manufacturer with fabrication, assembly and installation training.
B.	System Supplier to perform inspections as needed.
1.05	SUBMITTALS
A.	See Section 01 3000 - Administrative Requirements, for submittal procedures.
B.	Product Data:  Provide component dimensions.
C.	Shop Drawings: Indicate daylight opening dimensions and overall frame dimensions, window schedule and elevations.
D.	System Supplier's Product Data: Include complete Order and Fabrication manual extracts, maintenance and cleaning instructions.
1.06	QUALITY ASSURANCE
A.	System Supplier Manufacturer and Installer Qualifications:  Company specializing in fabrication of commercial sliding doors with not fewer than three years of experience.
1.07	DELIVERY, STORAGE, AND HANDLING
A.	Deliver products to project site and store in manufacturer's protective cartons until openings are ready for door installation.
B.	Protect finished surfaces with wrapping paper or strippable coating during installation.  Do not use adhesive papers or sprayed coatings that bond to substrate when exposed to sunlight or weather.
1.08	FIELD CONDITIONS
A.	Do not install sealants when ambient temperature is less than 40 degrees F (5 degrees C).
B.	Maintain this minimum temperature during and 24 hours after installation of sealants.
1.09	WARRANTY
A.	See Section 01 7800 - Closeout Submittals, for additional warranty documentation.
B.	Provide a two year material product warranty from the System Supplier starting on the date of delivery.
C.	Correct defective Work within a [   ] year period after Date of Substantial Completion.
D.	Provide [   ] year manufacturer warranty against failure of glass seal on insulating glass units, including interpane dusting or misting.  Include provision for replacement of failed units.
E.	Provide [   ] year manufacturer warranty against excessive degradation of exterior finish.  Include provision for replacement of units with excessive fading, chalking, or flaking.
F.	Provide a System Design Representation Statement from the System Supplier.

PART 2  PRODUCTS
2.01	ACCEPTABLE SYSTEM SUPPLIER PRODUCTS
A.	Basis of Design: Schuco (www.schuco-usa.com); Product: ASS 77 PD.HI – manually operated.
B.	Product Description: Thermally broken [double; triple] track aluminum framed sliding system integrated into [curtain wall; glass facade; masonry; metal stud; ___ opening]. Thermal breaks are to be constructed using Polyamide isobars. Pour and debridge thermal breaks are not acceptable. Glass to be factory glazed.
C.	Operating Types available in Sliding System:
1.	XX, (Type 2A): Double track, two sliding doors.
2.	XO, (Type 2A/1): Double track, one sliding door, one fixed lite.
3.	XOX, (Type 2B): Double track, two sliding doors, one fixed lite.
4.	OXO, (Type 2C): Double track, one sliding door, two fixed lites.
5.	XXXX, bi-parting (Type 2D): Double track, four sliding doors.
6.	OXXO, bi-parting (Type 2D/1): Double track, two sliding doors, two fixed lites.
7.	XXX (Type 3E): Triple track, three sliding doors.
8.	OXX (Type 3E/1): Triple track, two sliding doors, one fixed lite.
9.	OXXXXO, bi-parting (Type 3F): Triple track, four sliding doors, two fixed lites.

2.02	SLIDING DOORS
A.	Performance Requirements
1.	Aluminum vent framing to be mitered and factory assembled using corner cleats and chevrons to support, align as well as seal all profile joints. Outer frame framing can be [mitered; butt jointed].
2.	Outer frame depth:
a.	Double track: 7-3/4" (197 mm).
b.	Triple track: 11-11/16" (297 mm).
3.	Vent frame depth: 3-1/16" (77 mm).
4.	Isobar type: Polyamide.
5.	The positive design wind load of the project is [   ] psf ([   ] Pa). 
6.	The negative design wind load of the project is [   ] psf ([   ] Pa).
7.	Design and size sliding doors to withstand the following load requirements, when tested in accordance with ASTM E 330 using test loads equal to 1.5 times the design wind load with 10 second duration of maximum load.
8.	Member Deflection: Limit member deflection to L / 200 or a maximum of 9/16 inch (15 mm).
9.	Deflection: Maximum allowable deflection for any member supporting a single lite of glass: 9/16 inch (15 mm).
10.	Condensation Resistance Factor: For the frame of CRFf [   ] or better in accordance with AAMA 1503.
11.	U-value of glazed window assembly to be [   ] BTU/(h*sq ft* degrees F) ([   ] W/(sq meters*degrees K)) or better, as determined from NFRC 100 thermal performance test report or simulation.
12.	Acoustical performance: STC rating of [   ]. OITC rating of [   ].
13.	Life cycle Requirements: No damage to fasteners, hardware parts or other components that would render operable windows inoperable and no reduction in air and water infiltration resistance when tested according to AAMA 910. 
14.	Air and Vapor Seal: Maintain continuous air barrier and vapor retarder throughout assembly. 
15.	System Internal Drainage:  
a.	Single and Double track: Drain to the exterior by means of a weep drainage network for any water entering joints, condensation occurring in glazing channel, or migrating moisture occurring with system. 
16.	Forced Entry Resistance: Conform to ASTM F842 requirements for performance level Type A - Grade: 10.
B.	Sliding Door Type Specific Performance, Hardware and Accessory Requirements: 
1.	Sliding Door:
a.	Types:
1)	XX, XO (Type 2A, 2A/1): Double track 
(a)	Performance Class and Grade: Performance Class = AW, Performance Grade = 40 in accordance with AAMA/WDMA/CSA 101/I.S.2/A440.
(b)	Water Infiltration: No uncontrolled water ingress at a static pressure difference of 8 psf ([390] Pa) in accordance with ASTM E 283.
(c)	Air Infiltration and Exfiltration: Limit air infiltration through operable light assembly to 0.10 cu ft min/sq ft ([0.5] L/s*sq m) of wall area, measured at a differential of 6.27 psf (300 Pa) in accordance with ASTM E 283.
(d)  Canadian air infiltration/exfiltration level: A3.

b.	Proprietary System Supplier hardware and accessories to be used including: 
1)	Fully concealed multi-point locking.
2)	Weatherstrip type: brush seal.
3)	Handles: 
(a)	Type: [push bar; pull grip].
(b)	Color: Per System Supplier's options.
4)	Reinforcing (as necessary to achieve highest structural ratings):
(a)	internal: galvanized steel
(b)	external: galvanized steel
2.03	MATERIALS
A.	Extruded Aluminum: ASTM B221 (ASTM B221M), 6063 alloy, T6 temper.
B.	Gaskets: EPDM.
C.	Glazing: As specified in Section 08 8000.
2.04	FABRICATION
A.	Fabricate components with smallest possible clearances and shim spacing around perimeter of assembly.
B.	Accurately fit, secure and seal joints and corners using corner keys and epoxy glue.
C.	Prepare components to receive anchor devices.
D.	Provide internal drainage of glazing spaces to exterior through weep holes as per System Supplier's instructions.
E.	Factory or site glaze sliding door units.
2.05	FINISHES
A.	Class I Natural Finish or Anodized Plus Natural Anodized 2-step Finish:
1.	Class I Natural Anodized Finish:  AAMA 611 AA-M12C22A41 Clear anodic coating not less than 0.7 mils (0.018 mm) thick.
2.	Anodized Plus Natural Anodized Finish: AAMA 612 clear anodic coating with electrolytically deposited organic seal not less 0.7 mils (0.02 mm) thick; color as scheduled.
B.	Class II Natural Anodized Finish:  AAMA 611 AA-M12C22A31 Clear anodic coating not less than 0.4 mils (0.01 mm) thick.
C.	Class I Color Anodized Finish or Anodized Plus Color Anodized 2-step Finish:
1.	Class I Color Anodized Finish:  AAMA 611 AA-M12C22A42 Integrally colored anodic coating not less than 0.7 mils (0.018 mm) thick; light bronze.
2.	Anodized Plus Color Anodized Finish: AAMA 612 electrolytically deposited colored anodic coating with electrolytically deposited organic seal not less 0.7 mils (0.02 mm); color as scheduled.
D.	Class I Color Anodized Finish:  AAMA 611 AA-M12C22A44 Electrolytically deposited colored anodic coating not less than 0.7 mils (0.018 mm) thick; light bronze.
E.	Class II Color Anodized Finish:  AAMA 611 AA-M12C22A32 Integrally colored anodic coating not less than 0.4 mils (0.01 mm) thick; light bronze.
F.	Superior Performance Organic Coating System: AAMA 2605 multiple coat, thermally cured polyvinylidene fluoride system; color as scheduled.
G.	High Performance Organic Finish:  AAMA 2604;  multiple coats, thermally cured fluoropolymer system; color as scheduled.
H.	Pigmented Organic Coating System:  AAMA 2603; polyester or acrylic baked enamel finish; color as scheduled.
I.	Operator and Exposed Hardware:  Enameled to ________ color.
J.	Apply 1 coat of bituminous coating to concealed aluminum and steel surfaces in contact with dissimilar materials.
K.	Shop and Touch-Up Primer for Steel Components:  SSPC-Paint 25, zinc oxide, alkyd, linseed oil primer.
L.	Touch-Up Primer for Galvanized Steel Surfaces:  SSPC-Paint 20, zinc rich.
2.06	INSECT SCREEN FRAME
A.	Rolled aluminum frame of rectangular sections; fit with adjustable hardware; nominal size similar to operable glazed unit.
B.	Insect Screens: FS L-S-125, woven plastic mesh; [14/18; or    ] mesh size.
C.	Insect Screens: [14/18; or   ] mesh, [steel; aluminum; glass fiber; or   ] strands.
D.	Insect screens may be [sliding; hinged; fixed].
E.	Assemble insect screen frames with mitered and reinforce corners. Secure wire mesh tautly in frame. Fit frame with [four;   ], [spring loaded steel pin; or   ] retainers.
PART 3  EXECUTION
3.01	EXAMINATION
A.	Verify that wall or curtain wall openings and adjoining air and vapor seal materials are ready to receive aluminum framed glass sliding doors.
3.02	INSTALLATION
A.	Install door unit assembly and hardware in accordance with System Supplier's instructions.
B.	Attach frame and shims to perimeter opening to accommodate construction tolerances and other irregularities.
C.	Provide flat and level sub-sill for continuous support of frame sill.
D.	Use anchorage devices to securely fasten sliding door assembly to wall construction without distortion or imposed stresses.
E.	Install perimeter sealant in accordance with requirements of Section 07 9005.
F.	Install glass in fixed and sliding units in accordance with manufacturer's recommendations.
G.	Coordinate attachment and seal of perimeter air barrier and vapor retarder materials.
3.03	TOLERANCES
A.	Maintain dimensional tolerances and alignment with adjacent work.
B.	Maximum Variation from Plumb:  1/16 inch (1.5 mm).
C.	Maximum Variation from Level:  1/16 inch (1.5 mm).
D.	Longitudinal or Diagonal Warp:  Plus or minus 1/8 inch (3 mm) from 10 foot (3 m) straight edge.
3.04	FIELD QUALITY CONTROL
A.	Provide the services of the Manufacturer's field representative to observe installation and make report. 
B.	See Section 01 4000 - Quality Requirements, for general requirements for testing and inspection.
3.05	ADJUSTING
A.	Adjust hardware for smooth operation.
3.06	CLEANING
A.	Remove protective material from factory finished surfaces.
B.	Wash surfaces by method recommended and acceptable to sealant and window manufacturer; rinse and wipe surfaces clean.
C.	Remove excess sealant by moderate use of mineral spirits or other solvent acceptable to sealant manufacturer.
3.07	PROTECTION
A.	Protect installed products from damage during subsequent construction activities.
END OF SECTION

Disclaimer:  Schüco USA LLLP has written this sample specification as an aid to a professionally qualified design professional.  Schüco shall not be responsible for the use of this specification in project construction documents.  The use of this specification requires the sole professional judgment and expertise of a qualified design professional to adapt the information in this specification to the specific needs of the project, to coordinate with the construction documents, and to meet all applicable building codes, regulations and laws.  THEREFORE, SCHÜCO EXPRESSLY DISCLAIMS ANY IMPLIED WARRANTY INCLUDING THE WARRANTY OF MERCHANTABILITY OR FITNESS FOR PARTICULAR PURPOSE.

ASS 77 PD.HI MANUALLY OPERATED	08 3200 -  	SLIDING GLASS DOORS